Create your own texture:


1. Open "Custom1.jpg" or "Custom2.jpg"
2. Paint the lower side view within the JPG
3. Copy the lower side view, mirror it and shift it to the top within the JPG
--- By now, your texture would be finished. But with time and the many authors a little fault slipped into the texture mapping. So please continue with the next steps ---
4. Stretch the upper side view vertically to about 105%
5. Do not overlap the lower side view with the upper stretched side view.

6. Save the JPG.


Hint1: To check your textures => Just switch the textures in Heli-X, there is no need to load the helicopter every time.
Hint 2: Under Heli-X menue "Configuration" it is possible to assign a keyboard key for text switching.


Have fun :-) :-)

Rolf Rohner